
=====
INPUT
=====

Direct access to common input devices.  Each target has its own 
directory containing the implementations of the library's interface.

The zx spectrum target is the reference implementation -- new
implementations should consult that for example code.
