$Id: README,v 1.2 2001/04/18 13:21:37 stefano Exp $

Changed the (0:0) origin to top-left (hardware) to port easily the stuff.
The Z88 uses the window and closegfx commands that aren't supported 
with the other ports.

Spectrum, ZX81, VZ200/300, Jupiter ACE and TI calculators are supported
with all the others gfx commands.

