# core.math

Builtin mathematical intrinsics
Source:
License:
Boost License 1.0.
Authors:
, Don Clugston

pure nothrow @safe real cos(real x);
  Returns cosine of x. x is in radians.

  Special Values
  x | cos(x) | invalid?
  --- | --- | ---
  NAN | NAN | yes
  ±∞ | NAN | yes

  BUGS:
  Results are undefined if |x| >= 264.
pure nothrow @safe real sin(real x);
  Returns sine of x. x is in radians.

  Special Values
  x | sin(x) | invalid?
  --- | --- | ---
  NAN | NAN | yes
  ±0.0 | ±0.0 | no
  ±∞ | NAN | yes

  BUGS:
  Results are undefined if |x| >= 264.
pure nothrow @safe long rndtol(real x);
  Returns x rounded to a long value using the current rounding mode. If the integer value of x is greater than long.max, the result is indeterminate.
real rndtonl(real x);
  Returns x rounded to a long value using the FE_TONEAREST rounding mode. If the integer value of x is greater than long.max, the result is indeterminate.
pure nothrow @safe float sqrt(float x);
  Compute square root of x.

  Special Values
  x | sqrt(x) | invalid?
  --- | --- | ---
  -0.0 | -0.0 | no
  <0.0 | NAN | yes
  +∞ | +∞ | no

pure nothrow @safe double sqrt(double x);
  ditto
  Compute square root of x.

  Special Values
  x | sqrt(x) | invalid?
  --- | --- | ---
  -0.0 | -0.0 | no
  <0.0 | NAN | yes
  +∞ | +∞ | no

pure nothrow @safe real sqrt(real x);
  ditto
  Compute square root of x.

  Special Values
  x | sqrt(x) | invalid?
  --- | --- | ---
  -0.0 | -0.0 | no
  <0.0 | NAN | yes
  +∞ | +∞ | no

pure nothrow @safe real ldexp(real n, int exp);
  Compute n * 2exp
  References:
  frexp
pure nothrow @safe real fabs(real x);
  Returns |x|

  Special Values
  x | fabs(x)
  --- | ---
  ±0.0 | +0.0
  ±∞ | +∞

pure nothrow @safe real rint(real x);
  Rounds x to the nearest integer value, using the current rounding mode. If the return value is not equal to x, the FE_INEXACT exception is raised. nearbyint performs the same operation, but does not set the FE_INEXACT exception.
pure nothrow @safe real yl2x(real x, real y);
  Building block functions, they translate to a single x87 instruction.

Page generated by Ddoc. Copyright Digital Mars 2000 - 2011.